Current Help System: PC-DMIS NC (View Core Help)

### Step 2: Set the Work Offset

Using the
Operation | CNC Programming | Use Work Offset menu option, set the work offset for the part you will measure into the NC controller. Make a note of its number. PC-DMIS NC supports standard work offset registers. (Example G54-G59 for Fanuc style controls). The objective is to match up the initial PC-DMIS NC alignment with a work offset. In the case of a

- Heidenhain Controls: modify the Preset Table or Datum Table.

Next Step...