Current Help System: PC-DMIS Portable (View Core Help)

## Portable Toolbar

Portable Toolbar for Romer interface

The Portable Toolbar contains several icons that allow you to access various frequently used functions and windows that are helpful when programming or measuring with portable devices.

The available toolbar icons for Romer arms are described in this table:

Icon | Description
| Execute | Executes the measurement process for any currently marked feature(s). See "Execute" in the "Using Advanced File Options" section in the PC-DMIS Core help file.
| Execute Feature | Executes the selected feature. See "Execute Feature" in the "Using Advanced File Options" section in the PC-DMIS Core help file.
| Execute from Cursor | Executes the part program starting at the selected feature and then working down the Edit window. See "Execute From Cursor" in the "Using Advanced File Options" section in the PC-DMIS Core help file.
| Mark | Marks the selected feature with the specified mark color and prepares it for execution. See "Mark" in the "Editing a Part Program" section in the PC-DMIS Core help file.
| Mark All | Marks all features in the Edit window. See "Mark All" in the "Editing a Part Program" section.
| Clear Marked | Removes all highlights from currently marked features within the Edit window. See "Clear All" in the "Editing a Part Program" section in the PC-DMIS Core help file.
| Edit Dialog | Accesses the dialog box associated with the currently selected command if one exists.
| Import IGES Files | Begins the import operation for the IGES CAD file type (.igs or .iges). See "Importing an IGES File" in the "Using Advanced File Options" section in the PC-DMIS Core help file.
| Set Alignment | Links the CAD data to the measured data. See "CAD Equals Part" in the "Creating and Using Alignments" section in the PC-DMIS Core help file.
| Leap Frog Alignment | Performs a Leapfrog operation. See "Performing a Leapfrog Operation".
| Curve Mode | Places PC-DMIS into Curve mode (for use with wire-frame). See "Switching Between Curve and Surface Modes" in the "Editing the CAD Display" section in the PC-DMIS Core help file.
| Surface Mode | Places PC-DMIS into Surface mode (for use with surface data). See "Switching Between Curve and Surface Modes" in the "Editing the CAD Display" section in the PC-DMIS Core help file.
| Virtual Keyboard | Displays a Virtual Keyboard. See "Using the Virtual Keyboard" in the "Using Other Windows, Editors, and Tools" section in the PC-DMIS Core help file.
| Probe Readouts | Displays or hides the Probe Readout window. See "Using the Probe Readout Window" in the "Using Other Windows, Editors, and Tools" section in the PC-DMIS Core help file.
| Large Status Window | Displays or hides the Status window. See "Using the Status Window" in the "Using Other Windows, Editors, and Tools" section in the PC-DMIS Core help file.
| Report Window | Displays or hides the Report window. See "About the Report Window" in the "Reporting Measurement Results" section in the PC-DMIS Core help file.
| Auto Circle | This allows quick access to the Auto Feature dialog box without having all auto feature buttons on the screen. Once the Auto Feature dialog box is open, you can select another auto feature if needed.

Important: Different and additional icons are displayed on the Portable toolbar for Leica trackers.