Current Help System: PC-DMIS Settings Editor (View Core Help)

### DEA Wrist

Specifies whether a DEA CW43 or CW43L wrist is present or not. When this value is set to TRUE (1), capabilities for your infinite DEA wrist are enabled.

Important: In a Multiple Arm configuration you need to set the values on the Arm1 system for the other arm machines. For example: If you have a DEAWrist that is present on your Arm2 system, then you would need to set the DEAWrist option under Option_CMM2 to 1.

Entry Name: DEAWrist

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

Administrator permission is