Current Help System: PC-DMIS Settings Editor (View Core Help)

### Measure Mode

This option determines the mode that is used for dual arm calibration.

Entry Name: MeasureMode

Entry Type: Whole Number specifying calibration mode. Default value is 0.

Mode Key:

0 | Both arms measure tool. PC-DMIS will prompt you to measure each sphere position with both arms.
1 | First arm holds tool and second arm measures. PC-DMIS will prompt you to move the master arm to each position and then measure the spherical tool with the slave arm
2 | Second arm holds tool and first arm measures. PC-DMIS will prompt you to move the slave arm to each position and then measure the spherical tool with the master arm.