Current Help System: Tutor Translator (View Core Help)

#### Coaxiality

Tutor allows the following coaxiality command:

- Checked Line – Datum Line.

where:

- Line means Class Line feature: Line, Cylinder and Cone.

GEO_TOL(COAX,MEMORY[123],MEMORY[124]) translates to è

DIM COAX1=COAXIALITY FROM CYLINDER E.MEMORY[123].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=0.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[123].TP = COAX1.MEAS
ASSIGN/E.MEMORY[123].GTOL = 6
ASSIGN/E.WM1 = E.MEMORY[123]

GEO_TOL(>MEMORY[200],COAX,MEMORY[123],MEMORY[124]) translates to è

DIM COAX1=COAXIALITY FROM CYLINDER E.MEMORY[123].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=0.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = E.MEMORY[123]
ASSIGN/E.WM1.TP = COAX1.MEAS
ASSIGN/E.WM1.GTOL = 6
ASSIGN/E.MEMORY[200] = E.WM1

GEO_TOL DIST(COAX,MEMORY[123],MEMORY[124],6.) translates to è

DIM COAX1=COAXIALITY FROM CYLINDER E.MEMORY[123].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=12.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[123].TP = COAX1.MEAS
ASSIGN/E.MEMORY[123].GTOL = 6
ASSIGN/E.WM1 = E.MEMORY[123]

GEO_TOL DIST(COAX,MEMORY[123],MEMORY[124], DISTVAR) translates to è

Where the variable DISTVAR contains the dist value.

DIM COAX1=COAXIALITY FROM CYLINDER E.MEMORY[123].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH= DISTVAR*2 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[123].TP = COAX1.MEAS
ASSIGN/E.MEMORY[123].GTOL = 6
ASSIGN/E.WM1 = E.MEMORY[123]