Current Help System: Tutor Translator (View Core Help)

## Element Evaluation

Tutor evaluates element when it executes a direct or indirect measurement (Mxxx or Ixxx) command or when it executes an OUTPUT command. Evaluation is translated with a TUTOR_OUTPUT subroutine call.

SUBROUTINE/TUTOR_OUTPUT,TutorSub.prg
TE = : TUTOR ELEMENT STRUCTURE,
OFT = OFMT : TUTOR OUTPUT FORMAT TABLE,
TT = : THEORETICAL VALUES TABLE,
ELEMNAME = : NAME OF TUTOR ELEMENT STRUCTURE,

The evaluation of the element

MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",,,

The output layout is fixed. It is not possible to program the Headers, Footers, Titles, Vertical layouts or the Field order. Output labels are always given in English.