Current Help System: Tutor Translator (View Core Help)

### Slot Construction Commands

In PC-DMIS there is a command to construct a slot. Nevertheless the rules by which existing features can be used are completely different. Therefore it is not possible to use the same features from the Tutor part program.

It is not possible to translate the ISLOT command. As a partial solution the ISLOT command is translated to a constructed slot which construction features are undefined and theoretical values are forced to 0 unless theoretical values are available.( X, Y, Z, CX, CY, CZ, DM and DM2).

A Comment/Oper is added in order to notify the operator about missing compatibility with original Part Program.

Round Slot

ISLOT (MEMORY[10], 10, MEMORY[101]) ISLOT (MEMORY[10], 6, MEMORY[105])
ISLOT (MEMORY[10], 6, MEMORY[101], MEMORY[107], MEMORY[119], MEMORY[111], MEMORY[112],
MEMORY[105] translates to è

…
… Warning Messages
…

SLT1 =FEAT/SLOT,RECT,IN

THEO/<0,0,0>,<0,0,0>,0,0
ACTL/<0,0,0>,<0,0,0>,0,0
CONSTR/SLOT,ROUND SLOT,,

ASSIGN/E.WM2 = E.WM2
ASSIGN/E.WM1 = TUTORELEMENT("SLT1")
ASSIGN/E.MEMORY[10] = E.WM1
…
… Evaluation commands.
…

Square Slot

It is not possible to translate the ISLOT command. There is no PC-DMIS command for Square Slot construction.