Current Help System: Tutor Translator (View Core Help)

### Plane Construction Commands

IPL (MEMORY[42], 3, MEMORY[101])
IPL (MEMORY[42], 3, MEMORY[101], FORM LSM) translates to è

PLN11 =FEAT/PLANE,RECT

THEO/<152.0023,150.001,130.0007>,<-0.9999998,0.000073,-0.0005604>
ACTL/<152.0023,150.001,130.0013>,<-0.9999998,0.000073,-0.0005604>
CONSTR/PLANE,BF,E.MEMORY[101].ID,E.MEMORY[102].ID,E.MEMORY[103].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PLN11")
ASSIGN/E.MEMORY[42] = E.WM1
…
… Evaluation commands.
…

IPL (MEMORY [43], MEMORY[102],MEMORY[105],MEMORY[107])
IPL (MEMORY [43], MEMORY[102],MEMORY[105],MEMORY[107], FORM LSM) translates to è

PLN12 =FEAT/PLANE,RECT

THEO/<104.6677,121.3347,78.6673>,<-0.7149675,0.1935771,0.6718255>
ACTL/<104.6677,121.3347,78.6673>,<-0.7149675,0.1935771,0.6718254>
CONSTR/PLANE,BF,E.MEMORY[102].ID,E.MEMORY[105].ID,E.MEMORY[107].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PLN12")
ASSIGN/E.MEMORY[43] = E.WM1
…
… Evaluation commands.
…

The following commands that use ISO algorithm don’t have an equivalent PC-DMIS command. See the section on ”Construction Commands with no PC-DMIS Equivalent” for more information.

IPL (MEMORY [44], 3, MEMORY[101], FORM ISO)
IPL (MEMORY [43], MEMORY[102],MEMORY[105],MEMORY[107], FORM ISO)