Current Help System: PC-DMIS Vision (View Core Help)

### Measuring Auto Features with the NC-100 Video Probe

The Insert | Feature | Auto menu allows you to access to the Auto Feature (DCC) functions if an automatic CMM (Coordinate Measuring Machine) is being used. The Auto Features dialog box allows you to create any type of Auto Feature.

The main topics discussed in this section include:

- Auto Feature Functions Specific to NC 100 Video Probe

- Vector Point with NC-100

- Edge Point with NC-100

- Characteristic Points with NC-100

- Circle, Pin, or Baricenter with NC-100

- Round Slot with NC-100

- Square Slot/Gap & Flush with NC-100

On certain topics this manual will refer you to the "Creating Auto Features" section for more complete information.

Note: See the "Creating Auto Features" section for information on measuring Auto Features in general, but be aware that some options documented in that section may not be available when using the NC-100 Video probe.