Current Help System: PC-DMIS Vision (View Core Help)

### Vision Measuring Methods

PC-DMIS Vision offers three ways to measure parts in DCC Mode:

- CAD Selection Method: If you have a CAD drawing, you can program the entire part program offline based on the CAD drawing. You can then execute this program on a live machine. See “CAD Selection Method” for more info on this procedure.

- Target Selection Method: This method does not require a CAD drawing and is done entirely online using a live machine. See “Target Selection Method” for more information on this procedure.

- Auto Feature Guess Mode: Using the Quick Start window, you can begin taking hits and PC-DMIS will automatically guess the feature type. See "Auto Feature Guess Mode" for more information on this procedure.

More:

CAD Selection Method

Target Selection Method

Required Clicks for Supported Features

Auto Feature Guess Mode