Current Help System: PC-DMIS CMM (View Core Help)

#### Axis Basic Scan - Wire frame Data Method

Wire frame CAD data also can be used to generate points for a line. Click near the desired wire on the axis. PC-DMIS will highlight the entire selected wire. It will also fill up the Start Point and End Point items in the dialog box with the start an ending points of the selected wire.

CutVec: This vector is the normal vector of the Plane in which the straight line lies.