Current Help System: PC-DMIS CMM (View Core Help)

#### Move Speed

The Move Speed box allows you to specify the move speed for the PH9 calibration. Depending on the state of the Display absolute speeds check box in the Part/Machine tab of the Setup Options dialog box, the above Move Speed and Touch Speed boxes can either accept an absolute speed (mm/sec) or a percentage of the machine's defined top speed.

See "Move Speed %" in the "Setting your Preferences" section of the PC-DMIS Core documentation for additional ways to affect the speed in the measurement process.

Note: The number in the Move Speed box can contain no more than four decimal places. If a number with more than four decimal places is entered, PC-DMIS rounds the number off at the fourth decimal place.