#### Meas Width list

This list is available only on the Square Slot auto feature. | When you select Yes from Meas Width and then click the Create button, PC-DMIS will do the following during measurement:

- Measure two hits on the side of the slot.

- Adjust the angle vector.

- Measure two hits on the opposite side to calculate the width.

- Adjust the position of the last two hits at each end for the width.

Note: Generally, Square Slots only require five hits. With this option, however, taking six hits will yield a better measurement of the width.