### Setting Probe Depth on a Feature

To position the probe on a specific feature (i.e., a plane):

1. Move the cursor close to the feature.

2. Hold down the right mouse button.

3. Release the mouse button.

When the button is released, PC-DMIS will “snap” the probe to the closest CAD element and display the message: "Precise Depth Set on".

The status bar displays the current number of hits and the probe’s location.

Setting the Precise Probe Depth on a Feature