#### Void Detection Toggle

This icon only functions if you have Inspection Planner and IP Measure enabled on your portlock and if you are working with one of these supported features: Surface Point, Edge Point, Line, Plane, Circle, Cylinder, and Round Slot.

If selected, PC-DMIS detects hit targets that would normally occur in voids (empty spaces) on the CAD model and repositions them to a safe location, usually near the edge of the void.

This is often used with PC-DMIS Inspection Planner. See the "Void Detection" topic in the Inspection Planner documentation for additional information.