#### Creating Measured Features

1. From the Quick Start toolbar, select the Measure toolbar.

2. Click the icon of the feature you will measure. The top left icon on the dialog box changes to display what you will measure in this procedure and instructions appear on the status bar.

3. In offline mode, click the Program Mode icon from the PC-DMIS Modes toolbar. PC-DMIS draws a simulated depiction of the probe near the part in the Graphics Display window.

4. In offline mode, right click, to set the depth for the probe or in online mode. In online mode, move the probe to the desired depth.

5. Take the minimum number of hits on the part to measure the feature.

6. Click Finish or press Done on your jog box when the measurement is complete. The Quick Start dialog box remains open and PC-DMIS automatically compensates for probe radius and places the measured feature on the part in the Graphics Display window.

7. Follow steps four through six until you create all needed measured features.

8. Click Close when finished. The Quick Start dialog box closes.