## Inserting a Measured Feature

PC-DMIS allows you to insert measured features into your part program by interpreting your probe hits and guessing the correct feature type. If PC-DMIS guesses incorrectly, you can force PC-DMIS to choose the correct feature type as long as you have taken the minimum number of hits for the desired feature.

For information on creating the different feature types, consult the documentation set for your PC-DMIS configuration:

- PC-DMIS CMM

- PC-DMIS Portable

The procedures given in the following topic assume that you are working in offline mode.

More:

Guessing a Measured Feature Type

To Force the Insertion of a Certain Measured Feature Type