### MLB-110 Tip 0 not calibrated

An attempt was made to calibrate a tip other than the master tip (tip #0) when the calibration fixture's location relative to tip 0 was unknown. Tip 0 must be calibrated before any other tip can be calibrated. Note that this error may occur if a tip 0 calibration operation was started and then aborted.

Effect

Command is not executed.

What you should do

1. Calibrate tip 0.