### Importing STEP, VDAFS, and DXF/DWG Files

1. Select the File | Import menu option and then select STEP, VDAFS, DXF, or DWG. An Open dialog box appears.

2. Select the data type you want to import from the Files of Type list.

3. Navigate to the directory containing the file to import.

4. Click Import when ready to import the file. PC-DMIS will display the STEP Import dialog box.

STEP Import dialog box

Note: The import dialog boxes for the file types discussed in this topic are essentially the same as the STEP Import dialog box.

More:

Process Independent Entities

Reverse U-V Patch Order for Spline Surfaces