#### XYZ Point boxes

For a High Point feature, the XYZ Point boxes display the X, Y, and Z nominal for the start point.

After the new value is created, PC-DMIS will draw the animated probe at the new location. This location indicates the beginning position of the search. After the execution is complete, the XYZ point will contain the high point in the current workplane. Subsequent executions however will use the original start point for the search.

For all other feature types, the XYZ Point boxes display the X, Y, and Z nominal for the location of the feature.

After the new value is created, PC-DMIS will draw the animated probe at the new location. This location indicates where it will be taking the hit on the part.

For information on the X, Y, and Z axes check boxes, see the "Find Nearest CAD Element" topic.

Icon | Description
| Polar / Cartesian Toggle
| Find Nearest CAD Element
| Read Point from Machine
| Snap to Grid