Current Help System: PC-DMIS Laser (View Core Help)

#### Advanced Measurement Options Area

Best Fit Math Type

A Laser Auto Feature Circle also allows you to define the Best Fit Math Type. This is discussed in the "Best Fit Type" topic of the core PC-DMIS help file. Valid options for the Perceptron system are Maximum Inscribed, Minimum Circumscribed and Least Squares.

Relative to

This allows you to keep the relative position and orientation between a given feature (or features) and the auto feature. Click the button to open the Relative Feature dialog box to select the feature or features to which the auto feature is relative. Multiple features can be defined for each axis (XYZ) relative to your auto feature.