Current Help System: PC-DMIS Portable (View Core Help)

## Importing Nominal Data

PC-DMIS allows you to import nominal data of various types for the extraction of feature nominals.

Import the Following CAD Data Types:

- Standard Formats: DXF, IGES, SETP, STL, VDAFS, XYZ

- Optional: Catia 4, Catia 5, Parasolid, Pro-engineer, Unigraphics

- Direct CAD (DCI): ACIS, AIMS, CATIA, I-DEAS, Pro-engineer, Solidworks, Unigraphics

See "Importing CAD Data or Program Data" in the "Using Advanced File Options" section of the Core PC-DMIS help file.

If you have Inspection Planner programmed on your portlock, you may also use the Generic Parser to import ASCII files. See "Using the Generic Parser to Import ASCII Files" in the Core documentation for more information.