Current Help System: PC-DMIS Settings Editor (View Core Help)

### Light (0-3) Enabled

This option determines whether the light source is on or off for the 4 possible light sources. For each light source there are four lighting specifications that can be set (ambient, diffuse, position & specular). The light is enabled when the value is set to TRUE.

Entry Name: Light(0-3)_Enabled

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1 for Light 0. Default value is 0 for Light 1 -3.