Current Help System: PC-DMIS Settings Editor (View Core Help)

### Tesastar Infinite Wrist Type

Specifies whether some type of a Tesastar infinite wrist is present and if so, which type. When this value is set to 1 or 2, capabilities for the corresponding wrist type is enabled.

Entry Name: TesastarInfiniteWristType

Entry Type: Whole Number specifying Tesastar wrist type. Default value is 0.

Option Key:

0 | No Tesastar wrist is present.
1 | Indicates that a Tesastar CR wrist is present.
2 | Indicates that a Tesastar LW wrist is present.