Current Help System: PC-DMIS Settings Editor (View Core Help)

### Full Sphere Angle Check

This angle value determines whether or not PC-DMIS measures the entire sphere. If the difference between the shank vector and the probe vector is greater than this angle, then PC-DMIS measures the entire sphere. If not, the other parameters in the ProbeCal section will regulate the measurement pattern on the sphere.

Entry Name: FullSphereAngleCheck

Entry Type: Real Number specifying angle in degrees. The default is 25.