Current Help System: PC-DMIS Settings Editor (View Core Help)

### Offset From CAD

Determines whether an inserted Move Point will be offset along the CAD surface normal vector or the feature's vector. When this value is set to TRUE (1), the offset will be created in the CAD surface direction vector. The value is ignored if the "OffsetAlongTipVector" is set to TRUE (1).

Entry Name: OffsetFromCAD

Entry Type: Whole Number specifying Offset from CAD (1) or Offset from Feature (0). Default value is 1.