Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Use Theo Last State

This value tells PC-DMIS to use the theoretical information displayed in the dialog box when calculating the actual feature information from the measured data collected. This is useful when measuring cylinders with eight points (four high and four low). This can produce three valid measured cylinders at 90 degrees to one another. By using the theoretical information, it is possible to determine which of the three solutions is correct. This option is enabled when set to TRUE (1).

Entry Name: DCCUseTheoLastState

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.