Current Help System: PC-DMIS Settings Editor (View Core Help)

### Renishaw Calibration Order SP80

This value is used in conjunction with the "RenishawCalibrationCreateOrderSP600" and "RenishawCalibrationCreateOrderSP25" values to determine the order in which SP80 probe tips will be calibrated.

Entry Name: RenishawCalibrationOrderSP80

Entry Type: Whole Number to specify calibration order. Default value is 0.