Current Help System: PC-DMIS Settings Editor (View Core Help)

### Patch Dir Tech 2

This option determines the second technique that will be used for your Patch scan. Available options are Line or Body Axis. Using Line (0) technique, the approach of the probe is perpendicular to the line between the previous two hits. Using Body Axis (1) technique, the approach of the probe is perpendicular to the indicated axis (see PatchDirTech2Axis).

Entry Name: PatchDirTech2

Entry Type: Whole Number specifying Direction technique. Default value is 0.