Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Rotary

When this value is set to TRUE (1), Auto Rotary will automatically set the rotary table angle to get the most appropriate positioning of the part to measure the feature. This is typically used with stacked rotary tables.

Entry Name: AutoRotary

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.