Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Jump Holes

Determines whether or not the theoretical path should jump over holes and other hole-like features in the surface. When this option is set to TRUE (1), point data that does not lie within the selected surface (for example, hole features) will not appear in the Theoretical Path list and will be skipped during scan execution. When set to FALSE (0), the scan will scan into hole-like features.

Note: This is used with all scan but Perimeter and Freeform.

Entry Name: ScanDialogJumpHoles

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry