Current Help System: PC-DMIS Settings Editor (View Core Help)

### PTP_Auto Move

Allows you to define the default value for the Auto Move option that will be used when an Auto Feature is created. Auto Move commands can be inserted before, after or both for the created feature. The probe will move to a distance (PTP_AutoMoveDistance) above the centroid or first hit and last hit of the feature being created.

Entry Name: PTP_AutoMove

Entry Type: Whole Number to specify Auto Move option. Default value is 0.

Value Key:

0 | None
1 | Both
2 | Before
3 | After