Current Help System: PC-DMIS Settings Editor (View Core Help)

### Origin (PXYZ)

The Origin values are used to determine the length of the item to which thermal compensation is being applied.

Length = Current Position Value – Origin Value

- The X, Y, and Z values of the Origin boxes will be zero most of the time. However, some types of machines do not use zero for the origin of their scales.

- The Part value will typically also be zero unless there is some special type of fixturing constraint.

Entry Name: Origin(PXYZ)

Entry Type: Character String specifying origin location. Default value None ( ).

Number Key:

X | X Axis
Y | Y Axis
Z | Z Axis
P | Part