Current Help System: PC-DMIS Settings Editor (View Core Help)

### Edge Point Only Uses One Hit

When this value is set to TRUE (1), PC-DMIS normalizes the vectors for the edge point from the relevant CAD data. Therefore, only one hit is needed, where you would normally take multiple hits for an edge point.

Entry Name: EdgePointOnlyUsesOneHit

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.