Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Features – Initial Hits

Specifies the default Initial Hits value that will be used in the creation of Auto Features. Initial hits are used to measure the plane around the nominal point location for the specified feature. Initial sample hits are taken only on the initial measurement of the feature during execution of the part program. See the "Auto Features - Permanent Hits" topic.

Entry Name: DCC(Edge,Surf)InitHits

Entry Type: Whole Number to specify the number of Initial hits. Default values are 5 for Edge Points and 3 for Surf Points.