Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Focus Latency Duration 1

Provides the duration in seconds of the high speed focus latency calibration scan. If there are failures in the focus latency calibration, increasing the value slightly may allow successful processing.

Note: For optimal calibration results this values should be as small as practical and the difference between this value and "ProbeQualVisionOpticsCalFocusLatencyDuration2" should be large.

Entry Name: ProbeQualVisionOpticsCalFocusLatencyDuration1

Entry Type: Real Number specifying time in seconds. The default is 2.5.