Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Clip Right Percent

Provides the right edge of the clipping plane as a percentage of your laser sensor's field of view. The clipping plane allows you limit the amount of data that is collected form your laser sensor. For example, a value of 85 would eliminate the last fifteen percent form the right edge of the sensor's entire field of view, while a value of 100 will use all data up to the right edge of the sensor's field of view.

Entry Name: SensorClipRightPercent

Entry Type: Real Number to specify percentage. Default value is 0.