Current Help System: PC-DMIS Settings Editor (View Core Help)

### Measure Mode

This is a toggle field. This option displays the order of measuring the sample hits. The available choices are SURFACE(0), EDGE(1) or BOTH(2). This is only used when measuring Edge Points.

Entry Name: MeasureMode

Entry Type: Whole Number to specify Measure Mode. Default value is 0 (Surface).

Value Key:

0 | SURFACE | Takes sample hits on surface first and then on edge.
1 | EDGE | Takes sample hits on edge first and then on surface.
2 | BOTH | Takes sample hits on surface, then on edge and again on the surface.