Current Help System: PC-DMIS Settings Editor (View Core Help)

### Def Mode

When this option is set to TRUE (1), PC-DMIS will take the number of indicated hits around the spherical tool at either 10 or 15 degrees from the equator, plus one additional hit normal to the probe, 90 degrees from the equator. Otherwise, calibration occurs according to user defined parameters.

Entry Name: DefMode

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.