Current Help System: PC-DMIS CMM (View Core Help)

#### Touch Speed

The Touch Speed box allows you to specify the touch speed for the PH9 calibration. Depending on the state of the Display absolute speeds check box in the Part/Machine tab of the Setup Options dialog box, the above Move Speed and Touch Speed boxes can either accept an absolute speed (mm/sec) or a percentage of the machine's defined top speed.

See "Touch Speed %" in the "Setting your Preferences" section in the PC-DMIS Core documentation for additional information.

Note: The number in the Touch Speed box can contain no more than four decimal places. If a number with more than four decimal places is entered, PC-DMIS rounds the number off at the fourth decimal place.