Current Help System: PC-DMIS CMM (View Core Help)

## Performing Manual Scans with a Touch Trigger Probe

Manual TTP Scan dialog box

You can perform manual scans using a touch trigger probe (TTP).

To do this:

1. Place PC-DMIS into manual mode.

2. Access the Manual TTP Scan dialog box (Insert | Scan | Manual TTP).

3. Define the necessary parameters.

4. Click the Create button. PC-DMIS will display the Execution Mode Options dialog box and request that a hit be taken.

   Execution Mode Options dialog box

5. Take the hits as requested.

6. At the end of the scan, click the Scan Done button in the Execution Mode Options dialog box and PC-DMIS will stop the scan.

Note: Some scanning methods are not available when using a Touch Trigger Probe.