### MP-095 APC excessive entry speed

The APC controller has reported that the probe quill entered the rack at too high a speed.

What you should do

1. To clear the error, click Clear error in the XYZ Display window. To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, call your Giddings & Lewis service representative.