### MP-181 Invalid MEA data

MEA data has not been collected for this machine.

What you should do

1. To clear the error, click Clear error in the XYZ Display window. To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. Reload the configuration data with the correct configuration information from the CONFG disk.

3. If the error reoccurs, call your Giddings & Lewis service representative.