### MLB-161 APC rack could not be lowered

APC rack could not be lowered.

Effect

A command was executed which required the APC rack to be lowered and it could not be lowered.

What you should do

you should do

1. Check the command's definition and correct the part program.

2. Correct problem with the APC rack lower / raise capability.

3. If the error reoccurs, contact your Giddings & Lewis service representative.