### Changing Layout and Views

To change the screen layout and the orientation of the views:

1. Access the View Setup dialog box (Edit | Graphics Display Window | View Setup).

2. Select the desired screen style from the Layout area. For example, to split the screen into two different views of the part image, click on button two or three (in the first row). The window will be split horizontally or vertically, depending on the button that is chosen.

3. Using the drop-down list box, select the desired view orientation for each window that will be displayed. For example, to view the part image from the Z+ direction, simply select Z+ from the drop-down list box. Or, to view the same image from the Y- axis, select Y-. All of the display options only affect how PC-DMIS displays the part image. They do not affect the measured data or inspection results.

4. Select the Solid check box if you want to display your part in the selected view of your part as a solid. Leaving the check box blank will display the view of the part as a wire frame.

5. Click either the Apply button or the OK button.

1. - If the Apply button is selected, PC-DMIS will re-draw the Graphics Display window to reflect the current settings, allowing you to preview your changes.

   - If the OK button is selected, PC-DMIS will close the View Setup dialog box and apply the changes to the Graphics Display window. At any time before clicking OK, you can click Cancel to close the dialog box and revert the views to what they were.

More:

Change Size of Views