#### Changing Nominals Directly to Calculate Offsets

To enter new offset values:

1. Open the Line Offsets dialog box by clicking the Offset button from the Construct Line dialog box (Insert | Feature | Constructed | Line).

2. Select the Calculate Offsets option. The Nominals portion of the dialog box becomes editable.

3. Change the XYZ, IJK, or surface IJK values.

4. Click Calculate to update the offset values based on any nominals you've changed.

5. Click OK to save the offset.