### DOS to Windows

1. Using DOS, start up PC-DMIS for DOS. The Active Parts list will be displayed.

2. Click the POST button from the menu list.

3. Select the part program to be translated. PC-DMIS will display the Post Options menu.

4. Select the DIMS CMDS button (DIMS commands) from the menu list. PC-DMIS will ask for the Output File name.

5. Type the appropriate file name, followed by the three-character extension. It is suggested (but not mandatory) to use the extension ".dim".

6. When PC-DMIS is post processing the part program, it will ask you to enter the name of a PC-DMIS for Windows Probe File. Type the appropriate name.

7. Make sure that it is a probe file being used for Windows.

8. Press the ENTER key.

9. When the post processing is complete, PC-DMIS will display a message asking you to press any key to continue. PC-DMIS will then return to the Active Parts list.

10. Exit out of PC-DMIS for DOS.