## Inserting a Move Increment Command

The Insert | Move | Move Increment... menu option displays the Move Increment dialog box. You will use this dialog box to define the move increment command before you insert it into your part program.

Move Increment dialog box

When you click OK, PC-DMIS will insert the Move Increment command.

The Edit window command line for a Move Increment would read:
MOVE/INCREMENT, x, y, z

When PC-DMIS encounters this command it moves the probe the indicated XYZ distance (not an XYZ location as in a MOVE/POINT command). You must select the Store Move check box for this command to appear in the Edit window.

More:

XYZ Move

Store Move

OK to Move