## Dimensioning Perpendicularity

Looking for XactMeasure GD&T dimensions? If so, see:

- Using Feature Control Frames
- GD&T Dialog Box

Dimension Perpendicularity dialog box

The Insert | Dimension | Perpendicularity menu option measures the perpendicularity between two features. The second feature is always the datum feature. When only one feature is selected, the current working plane becomes the datum feature. This dimension type is considered one sided, meaning a single positive value tolerance is applied.

More:

To Dimension a Feature Using the PERPENDICULARITY Option:

Plus Tolerance for Perpendicularity Dimensions

Projected Distance for Perpendicularity Dimensions