### To Dimension a Feature Using the STRAIGHTNESS Option:

1. Select Insert | Dimension | Straightness from the submenu. The Straightness dialog box appears.

2. Select the feature(s) to dimension from the Feature List box.

3. Type the plus tolerance value in the Plus box.

4. Select either Inch or MM in the Units section.

5. Select where to output the dimension information. Select the Statistics, Report, Both, or None option.

6. Select the optional Display check box if you want to view dimension information in the Graphics Display window.

7. Select the desired Analysis options by marking the Textual check box or the Graphical check box. If the Graphical check box was marked, enter the Multiplier value in the Multiplier box.

8. If desired, select the Display check box in the Dimension Info area and click Edit to select the Dimension Info Format you would like displayed in the Graphics Display window.

9. Click the Create button.

The dimension will appear in the Edit window with this information:

dimension_name = STRAIGHTNESS,OF feat_1

AX | NOM | +TOL | -TOL | MEAS | MAX | MIN | DEV | OUT-TOL
M | 0.0000 | 0.0100 | 0.0100 | 5.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000